IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and Archicad 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "C:\ARCHITEKTURA II_SEM II\SYNAGGOGA\03_srm_model\SY_Mogielnica_IFC.ifc"
Time stamp: "2023-09-13T00:33:16"
Author: "Architect"
Organization: "Technical University of Lodz"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "IFC file generated by Graphisoft Archicad 26.0.0 POL FULL Windows version (IFC add-on version: 3001 POL FULL)."
Authorization: "The authorising person"
Application: "Archicad" version "26.0.0" identifier "IFC add-on version: 3001 POL FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Niezdefiniowane" id "https://orcid.org/0009-0003-2869-2715" (roles: "Student"; telecom address "Adres telecom projektanta": e-mail "223524@edu.p.lodz.pl") of Organization "Technical University of Lodz" (telecom address "Adres telecom projektanta": e-mail "223524@edu.p.lodz.pl")
  Owner history of Person "Niezdefiniowane" id "https://orcid.org/0009-0003-2869-2715" (roles: "Student"; telecom address "Adres telecom projektanta": e-mail "223524@edu.p.lodz.pl") of Organization "Technical University of Lodz" (telecom address "Adres telecom projektanta": e-mail "223524@edu.p.lodz.pl") | application "Archicad" version "26.0.0" identifier "IFC add-on version: 3001 POL FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change NOCHANGE | created 1694557995 (2023-09-12T22:33:15Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: USD
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "3D Reconstruction of Mogielnica Synagogue (1856-1939)"
  IFCSITE "Mogielnica" | latitude 52° 15′ 0″ | longitude 21° 0′ 0″ | elevation above sea level 0. | postal address: "Dol Square", "10", "Mogielnica", "Masovian", "05-640", "Poland" | description "https://www.geonames.org/764502/"
    IFCBUILDING "Synagogue" | postal address: "Dol Square", "10", "Mogielnica", "Masovian", "05-640", "Poland" | description "https://pl.wikipedia.org/wiki/Synagoga_w_Mogielnicy"
      IFCBUILDINGSTOREY "Poziom -1" | elevation -480.
        contains 207 elements
          124 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "KONSTRUKCYJNE" | names: "300375669", "300266806", "Bimah" | material: "KONSTRUKCYJNE" | property sets: AC_Pset_RenovationAndPhasing
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "Słupek Bimah 140 x 140" | names: "S2", "300375669" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 170" | FLOOR | names: "P1" | material: layers "Drewno konstrukcyjne 170" ("Drewno konstrukcyjne" 170.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 240 x 240" | names: "S1" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE200 (3) 240 x 443" | names: "300001643" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Nowy profil 240 x 240" | names: "S3" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          2 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 300 x 300" | names: "B1", "B4" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 350 x 300" | names: "B3" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          36 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Drewno konstrukcyjne" | names: "300375669" | material: "Drewno konstrukcyjne" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCWALL | type IFCWALLTYPE "Interior Wall 200 x 4870" | names: "300002538" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Drzwi podwójne 26" | names: "300002818" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Drzwi podwójne 26" | names: "300002818" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 150 x 300" | names: "B4" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCWALL | type IFCWALLTYPE "Deskowanie stropu 9315 x 100" | names: "300002031" | parts: 7 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 175 x 300" | names: "B3" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 220 x 220" | names: "S3" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE200 (4) 202 x 373" | names: "300001643" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          4 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 50 x 120" | names: "B0" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "Poziom 0" | elevation 0.
        contains 136 elements
          4 x IFCWALL | type IFCWALLTYPE "Ściana zewnętrzna 2 deskowanie 20 x 4430" | names: "300002523" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 240 x 150" | names: "S1" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 150 x 240" | names: "S1" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE200 (3) 240 x 443" | names: "300001643" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          9 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 50" | FLOOR | names: "300001643", "300266806", "300375669" | material: layers "Drewno konstrukcyjne 50" ("Drewno konstrukcyjne" 50.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Słup duży 320 x 320" | names: "300001571" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 150 x 300" | names: "B5" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          23 x IFCRAILING | type IFCRAILINGTYPE "Typ balustrady" | names: "300375669", "300073693", "300266806" | parts: 252 IFCBUILDINGELEMENTPART | property sets: Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_RailingCommon
          14 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Drewno konstrukcyjne" | names: "300375669", "300001571" | material: "Drewno konstrukcyjne" | property sets: AC_Pset_RenovationAndPhasing
          14 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "KONSTRUKCYJNE" | names: "300266806", "300375669" | material: "KONSTRUKCYJNE" | property sets: AC_Pset_RenovationAndPhasing
          3 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 20" | FLOOR | names: "300266806" | material: layers "Drewno konstrukcyjne 20" ("Drewno konstrukcyjne" 20.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 150" | FLOOR | names: "P2" | material: layers "Drewno konstrukcyjne 150" ("Drewno konstrukcyjne" 150.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          5 x IFCSTAIR | names: "300003228", "300266806", "300375669" | parts: 61 IFCMEMBER, 10 IFCBUILDINGELEMENTPROXY | property sets: Pset_ConcreteElementGeneral, Pset_StairCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          3 x IFCWALL | type IFCWALLTYPE "Ściana zewnętrzna 2 200 x 4430" | names: "300002523" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Okno dwuskrzydłowe 26" | names: "300002944" | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCWALL | type IFCWALLTYPE "Ściana zewnętrzna 200 x 4700" | names: "300002523" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          6 x IFCWINDOW | type IFCWINDOWSTYLE "Arch Window 3" | names: "300002944" | parts: 12 IFCBUILDINGELEMENTPART | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Okno dwuskrzydłowe 26" | names: "300002944" | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Door 4" | names: "300002818" | material: "Drewno konstrukcyjne" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCSLAB | type IFCSLABTYPE "Podłoga drewniana 90" | FLOOR | names: "P2" | material: layers "Podłoga drewniana" ("Drewno konstrukcyjne" 90.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Słup duży baza 360 x 360" | names: "300001571" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          9 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 100" | FLOOR | names: "300001571", "300001643" | material: layers "Drewno konstrukcyjne 100" ("Drewno konstrukcyjne" 100.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 320" | FLOOR | names: "Wallhole" | material: layers "Drewno konstrukcyjne 320" ("Drewno konstrukcyjne" 320.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 160" | FLOOR | names: "Wallhole" | material: layers "Drewno konstrukcyjne 160" ("Drewno konstrukcyjne" 160.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 70" | FLOOR | names: "300001643" | material: layers "Drewno konstrukcyjne 70" ("Drewno konstrukcyjne" 70.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Ściana drewniana_odniesienie cienka 80" | names: "300002535" | material: layers "Ściana drewniana_odniesienie cienka" ("Drewno konstrukcyjne" 80.) | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Drzwi 26" | names: "300002818" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Drzwi podwójne 26" | names: "300002818" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Door 1" | names: "300002818" | material: "Drewno konstrukcyjne" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "Poziom +1" | elevation 0.
        contains 211 elements
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 120 x 120" | names: "S7" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          129 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "KONSTRUKCYJNE" | names: "300266806", "300375669", "Bimah" (+5 more) | material: "KONSTRUKCYJNE" | property sets: AC_Pset_RenovationAndPhasing
          56 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Drewno konstrukcyjne" | names: "300375669", "300001643" | material: "Drewno konstrukcyjne" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 222 x 222" | names: "S4" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          6 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 70" | FLOOR | names: "300001643" | material: layers "Drewno konstrukcyjne 70" ("Drewno konstrukcyjne" 70.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 50 x 120" | names: "B0" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 180 x 150" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
      IFCBUILDINGSTOREY "Poziom +2" | elevation 4700.
        contains 262 elements
          13 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 160 x 120" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          164 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 100 x 80" | names: "300052264" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 180 x 150" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 180 x 200" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          6 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 150 x 100" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          16 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 100" | ROOF | names: "300014897" | material: layers "Drewno konstrukcyjne 100" ("Drewno konstrukcyjne" 100.); "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 150 x 200" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          10 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 120 x 120" | names: "300052264", "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 100 x 100" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          4 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 250 x 300" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "Drewno konstrukcyjne 120 x 120" | names: "S7" | material: "Drewno konstrukcyjne" | property sets: Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 250 x 130" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 150 x 300" | names: "B6" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 200 x 300" | names: "300001497" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "KONSTRUKCYJNE" | names: "Roof" | material: "KONSTRUKCYJNE" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 200 x 125" | names: "B6" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 400 x 150" | names: "B6" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          16 x IFCBEAM | type IFCBEAMTYPE "Drewno konstrukcyjne 80 x 60" | names: "300052264" | material: "Drewno konstrukcyjne" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCSLAB | type IFCSLABTYPE "Drewno konstrukcyjne 80" | ROOF | names: "300014897" | material: layers "Drewno konstrukcyjne 80" ("Drewno konstrukcyjne" 80.) | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Drewno konstrukcyjne" | names: "Roof" | material: "Drewno konstrukcyjne" | property sets: AC_Pset_RenovationAndPhasing

Types
  IFCBUILDINGELEMENTPROXYTYPE "KONSTRUKCYJNE" | 269 occurrences
  IFCCOLUMNTYPE "Słupek Bimah 140 x 140" | 16 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 170" | FLOOR | 1 occurrence
  IFCCOLUMNTYPE "Drewno konstrukcyjne 240 x 240" | 2 occurrences
  IFCCOLUMNTYPE "IPE200 (3) 240 x 443" | 6 occurrences
  IFCCOLUMNTYPE "Nowy profil 240 x 240" | 2 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 300 x 300" | 2 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 350 x 300" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Drewno konstrukcyjne" | 108 occurrences
  IFCWALLTYPE "Interior Wall 200 x 4870" | 1 occurrence
  IFCDOORSTYLE "Drzwi podwójne 26" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | property sets: Door Lining Properties, Door Panel Properties - Panel 1, Door Panel Properties - Panel 2
  IFCDOORSTYLE "Drzwi podwójne 26" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | property sets: Door Lining Properties, Door Panel Properties - Panel 1, Door Panel Properties - Panel 2
  IFCBEAMTYPE "Drewno konstrukcyjne 150 x 300" | 3 occurrences
  IFCWALLTYPE "Deskowanie stropu 9315 x 100" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 175 x 300" | 1 occurrence
  IFCCOLUMNTYPE "Drewno konstrukcyjne 220 x 220" | 2 occurrences
  IFCCOLUMNTYPE "IPE200 (4) 202 x 373" | 6 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 50 x 120" | 6 occurrences
  IFCWALLTYPE "Ściana zewnętrzna 2 deskowanie 20 x 4430" | 4 occurrences
  IFCCOLUMNTYPE "Drewno konstrukcyjne 240 x 150" | 6 occurrences
  IFCCOLUMNTYPE "Drewno konstrukcyjne 150 x 240" | 9 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 50" | FLOOR | 9 occurrences
  IFCCOLUMNTYPE "Słup duży 320 x 320" | 4 occurrences
  IFCRAILINGTYPE "Typ balustrady" | 23 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 20" | FLOOR | 3 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 150" | FLOOR | 1 occurrence
  IFCWALLTYPE "Ściana zewnętrzna 2 200 x 4430" | 3 occurrences
  IFCWINDOWSTYLE "Okno dwuskrzydłowe 26" | DOUBLE_PANEL_VERTICAL | 3 occurrences | property sets: Window Lining Properties, Window Panel Properties - Panel 1, Window Panel Properties - Panel 2
  IFCWALLTYPE "Ściana zewnętrzna 200 x 4700" | 3 occurrences
  IFCWINDOWSTYLE "Arch Window 3" | 6 occurrences
  IFCWINDOWSTYLE "Okno dwuskrzydłowe 26" | DOUBLE_PANEL_VERTICAL | 3 occurrences | property sets: Window Lining Properties, Window Panel Properties - Panel 1, Window Panel Properties - Panel 2
  IFCDOORSTYLE "Door 4" | 1 occurrence
  IFCSLABTYPE "Podłoga drewniana 90" | FLOOR | 3 occurrences
  IFCCOLUMNTYPE "Słup duży baza 360 x 360" | 4 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 100" | FLOOR | 9 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 320" | FLOOR | 1 occurrence
  IFCSLABTYPE "Drewno konstrukcyjne 160" | FLOOR | 1 occurrence
  IFCSLABTYPE "Drewno konstrukcyjne 70" | FLOOR | 7 occurrences
  IFCWALLTYPE "Ściana drewniana_odniesienie cienka 80" | 1 occurrence
  IFCDOORSTYLE "Drzwi 26" | SINGLE_SWING_RIGHT | 1 occurrence | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCDOORSTYLE "Drzwi podwójne 26" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | property sets: Door Lining Properties, Door Panel Properties - Panel 1, Door Panel Properties - Panel 2
  IFCDOORSTYLE "Door 1" | 1 occurrence
  IFCCOLUMNTYPE "Drewno konstrukcyjne 120 x 120" | 30 occurrences
  IFCCOLUMNTYPE "Drewno konstrukcyjne 222 x 222" | 2 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 180 x 150" | 3 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 160 x 120" | 13 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 100 x 80" | 164 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 180 x 200" | 2 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 150 x 100" | 6 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 100" | ROOF | 16 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 150 x 200" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 120 x 120" | 10 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 100 x 100" | 2 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 250 x 300" | 4 occurrences
  IFCBEAMTYPE "Drewno konstrukcyjne 250 x 130" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 200 x 300" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 200 x 125" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 400 x 150" | 1 occurrence
  IFCBEAMTYPE "Drewno konstrukcyjne 80 x 60" | 16 occurrences
  IFCSLABTYPE "Drewno konstrukcyjne 80" | ROOF | 2 occurrences

Property sets
  AC_Pset_RenovationAndPhasing | properties | on 811 objects (311 IFCBUILDINGELEMENTPROXY, 238 IFCBEAM, 89 IFCCOLUMN, 61 IFCMEMBER)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 76 objects (76 IFCBUILDINGELEMENTPROXY)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 398 objects (238 IFCBEAM, 89 IFCCOLUMN, 53 IFCSLAB, 12 IFCWALL)
    ConstructionType = "-" (IFCLABEL)
    FireRating = "-" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 335 objects (238 IFCBEAM, 89 IFCCOLUMN, 6 IFCWINDOW, 2 IFCDOOR)
    FireResistanceRating = "-" (IFCLABEL)
    IsCombustible = FALSE (IFCBOOLEAN)
  Pset_FireRatingProperties | properties | on 84 objects (61 IFCMEMBER, 23 IFCRAILING)
    IsCombustible = FALSE (IFCBOOLEAN)
  Pset_FireRatingProperties | properties | on 71 objects (53 IFCSLAB, 12 IFCWALL, 5 IFCSTAIR, 1 IFCWALLSTANDARDCASE)
    FireResistanceRating = "-" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 10 objects (6 IFCWINDOW, 4 IFCDOOR)
    FireResistanceRating = "" (IFCLABEL)
    IsCombustible = FALSE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 30 objects (30 IFCCOLUMN)
    Reference = "Drewno konstrukcyjne 120 x 120" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 10 objects (10 IFCCOLUMN)
    Reference = "Słupek Bimah 140 x 140" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 9 objects (9 IFCCOLUMN)
    Reference = "Drewno konstrukcyjne 150 x 240" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE200 (3) 240 x 443" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE200 (4) 202 x 373" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Słupek Bimah 140 x 140" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    Reference = "Drewno konstrukcyjne 240 x 150" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Słup duży 320 x 320" (IFCIDENTIFIER)
  Pset_ColumnCommon: 5 more contents on 12 objects not shown
  Pset_SlabCommon | properties | on 53 objects (53 IFCSLAB)
    AcousticRating = "0,00" (IFCLABEL)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_BeamCommon | properties | on 164 objects (164 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 100 x 80" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 16 objects (16 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 80 x 60" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 13 objects (13 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 160 x 120" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 120 x 120" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    Reference = "Drewno konstrukcyjne 50 x 120" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 150 x 100" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    Reference = "Drewno konstrukcyjne 150 x 300" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    FireRating = "-" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Drewno konstrukcyjne 180 x 150" (IFCIDENTIFIER)
  Pset_BeamCommon: 12 more contents on 17 objects not shown
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    FireRating = "-" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.7812 (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    SecurityRating = "-" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireExit = FALSE (IFCBOOLEAN)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    SecurityRating = "-" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    SecurityRating = "-" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireExit = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.7812 (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "-" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireExit = FALSE (IFCBOOLEAN)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "-" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorWindowGlazingType | properties | on 18 objects (12 IFCWINDOW, 6 IFCDOOR)
    IsCoated = FALSE (IFCBOOLEAN)
    IsLaminated = FALSE (IFCBOOLEAN)
    IsTempered = FALSE (IFCBOOLEAN)
    IsWired = FALSE (IFCBOOLEAN)
  Pset_ManufacturerOccurrence | properties | on 10 objects (6 IFCWINDOW, 4 IFCDOOR)
    BarCode = "-" (IFCIDENTIFIER)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerOccurrence | properties | on 8 objects (6 IFCWINDOW, 2 IFCDOOR)
    BarCode = "-" (IFCIDENTIFIER)
    SerialNumber = "-" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 10 objects (6 IFCWINDOW, 4 IFCDOOR)
    Manufacturer = "" (IFCLABEL)
    ModelLabel = "-" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 8 objects (6 IFCWINDOW, 2 IFCDOOR)
    Manufacturer = "-" (IFCLABEL)
    ModelLabel = "-" (IFCLABEL)
    ProductionYear = "dd.mm.rrrr" (IFCLABEL)
  Pset_RailingCommon | properties | on 15 objects (15 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_RailingCommon | properties | on 8 objects (8 IFCRAILING)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    FireRating = "-" (IFCLABEL)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 5. (IFCCOUNTMEASURE)
    NumberOfTreads = 5. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 160. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "-" (IFCLABEL)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    NumberOfRiser = 3. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 166.666666667 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "-" (IFCLABEL)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    NumberOfRiser = 12. (IFCCOUNTMEASURE)
    NumberOfTreads = 12. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 177.616666667 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "-" (IFCLABEL)
    HasNonSkidSurface = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 7. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 160. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_WindowCommon | properties | on 6 objects (6 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.38 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    SmokeStop = FALSE (IFCBOOLEAN)
  Door Lining Properties | predefined | on 4 type objects
  Door Panel Properties - Panel 1 | predefined | on 4 type objects
  Door Panel Properties - Panel 2 | predefined | on 3 type objects
  Window Lining Properties | predefined | on 2 type objects
  Window Panel Properties - Panel 1 | predefined | on 2 type objects
  Window Panel Properties - Panel 2 | predefined | on 2 type objects